From 7dfcc480ba1e19bd3232349fc733caef94034292 Mon Sep 17 00:00:00 2001
From: stainer_t <thomas.stainer@oecd-nea.org>
Date: Mon, 8 Sep 2025 13:48:49 +0200
Subject: Initial commit from Polytechnique Montreal

---
 doc/IGE335/Section3.15.tex | 96 ++++++++++++++++++++++++++++++++++++++++++++++
 1 file changed, 96 insertions(+)
 create mode 100644 doc/IGE335/Section3.15.tex

(limited to 'doc/IGE335/Section3.15.tex')

diff --git a/doc/IGE335/Section3.15.tex b/doc/IGE335/Section3.15.tex
new file mode 100644
index 0000000..9f320e9
--- /dev/null
+++ b/doc/IGE335/Section3.15.tex
@@ -0,0 +1,96 @@
+\subsection{The \moc{PSP:} module}\label{sect:PSPData}
+
+\begin{GuideUpdate}{3.04}
+
+The \moc{PSP:} module  is used to generate a graphical file in a PostScript
+ASCII format for  a DRAGON 2--D geometry which can be analyzed using the \moc{EXCELT:} tracking module
+(see \Sectand{TRKData}{descexcel}). The module \moc{PSP:} is based on the PSPLOT FORTRAN library from Nova
+Southeastern University.\cite{PSPLOT} Since only a few routines PSPLOT routines were required 
+and because additional PostScript routine not present in the original package were needed, the
+routines have been  completely readapted to DRAGON. These routines are no longer machine dependent
+and are now Y2K safe. The PostScript files generated by DRAGON can be viewed by any PostScript
+viewer, such as Ghostview\cite{GHOSTVIEW} or sent to a printer compatible with this language. In
+DRAGON the
+\moc{PSP:} module is activated using the following list of commands:
+
+\begin{DataStructure}{Structure \dstr{PSP:}}
+\dusa{PSGEO} \moc{:=} \moc{PSP:} $[$ \dusa{PSGEO} $]~\{$ \dusa{GEONAM} $|$ \dusa{TRKNAM} $\}$ $[$ \dusa{FLUNAM} $]$
+\moc{::} \dstr{descpsp}
+\end{DataStructure}
+
+\noindent 
+where
+
+\begin{ListeDeDescription}{mmmmmmmm}  
+
+\item[\dusa{PSGEO}] \texttt{character*12} name of the file
+that will contain the graphical description in a POSTSCRIPT format. This file must have a sequential
+ASCII format.
+
+\item[\dusa{GEONAM}] \texttt{character*12} name of a read-only \dds{geometry} (see \Sect{GEOData}).
+
+\item[\dusa{TRKNAM}] \texttt{character*12} name of an EXCELL type read-only \dds{tracking} (see \Sect{TRKData}).
+
+\item[\dusa{FLUNAM}] \texttt{character*12} name of an optional read-only \dds{fluxunk} (see \Sect{FLUData}). It is
+required only if a flux mapping plot is requested.
+
+\item[\dstr{descpsp}] structure containing the input data to this module (see \Sect{descpsp}).
+
+\end{ListeDeDescription}
+
+
+\subsubsection{Data input for module \moc{PSP:}}\label{sect:descpsp}
+
+\begin{DataStructure}{Structure \dstr{descpsp}}
+$[$ \moc{EDIT} \dusa{iprint} $]$ \\
+$[$ \moc{FILL} $\{$ \moc{NONE} $|$ \moc{GRAY} $|$ \moc{RGB} $|$ \moc{CMYK} $|$ \moc{HSB} $\}$ 
+$[$ \moc{NOCONTOUR} $]$ $]$\\
+$[$ \moc{TYPE} $\{$ \moc{REGION}  $|$ \moc{MIXTURE} $|$ \moc{FLUX} $|$ \moc{MGFLUX} $\}$ $]$ 
+\end{DataStructure}
+
+\noindent
+where
+
+\begin{ListeDeDescription}{mmmmmmmm}   
+
+\item[\moc{EDIT}] keyword used to modify the print level \dusa{iprint}.
+
+\item[\dusa{iprint}] index used to control the printing in this module.
+It must be set to 0 if no printing on the output file is required. 
+
+\item[\moc{FILL}] keyword to specify the drawing options.
+
+\item[\moc{NONE}] keyword to specify that only region contour are to be
+drawn.                                                                            
+
+\item[\moc{GRAY}] keyword to specify that the regions will be filled with various levels of
+gray.                                                                            
+
+\item[\moc{RGB}] keyword to specify that the regions will be filled with various colors taken using
+the RGB color scheme.                                                                            
+
+\item[\moc{CMYK}] keyword to specify that the regions will be filled with various colors taken
+using the CMYK color scheme. 
+
+\item[\moc{HSB}] keyword to specify that the regions will be filled with various colors taken
+using the HSB color scheme. This is the default option.                                                      
+
+\item[\moc{NOCONTOUR}] keyword to specify that the contour lines delimiting each region will not be drawn.
+
+\item[\moc{TYPE}] keyword to specify the type of graphics generated.
+
+\item[\moc{REGION}] keyword to specify that different colors or gray levels will be associated with each
+region. This is the default option.
+
+
+\item[\moc{MIXTURE}] keyword to specify that different colors or gray levels will be associated with each
+mixture.
+
+\item[\moc{FLUX}] keyword to specify that the group integrated flux is to be drawn.
+
+\item[\moc{MGFLUX}] keyword to specify that the group flux is to be drawn.
+
+\end{ListeDeDescription}
+   
+\end{GuideUpdate}
+\eject
-- 
cgit v1.2.3

