From 7dfcc480ba1e19bd3232349fc733caef94034292 Mon Sep 17 00:00:00 2001
From: stainer_t <thomas.stainer@oecd-nea.org>
Date: Mon, 8 Sep 2025 13:48:49 +0200
Subject: Initial commit from Polytechnique Montreal

---
 doc/IGE335/Section3.50.tex | 82 ++++++++++++++++++++++++++++++++++++++++++++++
 1 file changed, 82 insertions(+)
 create mode 100644 doc/IGE335/Section3.50.tex

(limited to 'doc/IGE335/Section3.50.tex')

diff --git a/doc/IGE335/Section3.50.tex b/doc/IGE335/Section3.50.tex
new file mode 100644
index 0000000..e2c10df
--- /dev/null
+++ b/doc/IGE335/Section3.50.tex
@@ -0,0 +1,82 @@
+\subsection{The \tt{PSP:} module}\label{sect:PSPData}
+
+The \moc{PSP:} module is used to generate a graphical file in a PostScript ASCII format for a DRAGON 2-D
+geometry which can be analyzed using the \moc{EXCELT:} or \moc{NXT:} tracking module (see Sections.~\ref{sect:EXCELLData}
+and~\ref{sect:NXTData}). The module \moc{PSP:} 
+is based on the PSPLOT Fortran library from Nova Southeastern University.\cite{PSPLOT} Since only a few
+PSPLOT routines were required and because additional PostScript routine not present in the original package were 
+needed, the routines have been completely readapted to DRAGON. These routines are no longer machine dependent.
+The PostScript files generated by DRAGON can be viewed by any PostScript viewer, such as Ghostview\cite{GHOSTVIEW}
+or sent to a printer compatible with this language. In DRAGON the \moc{PSP:} module is activated using the following 
+list of commands:
+
+\begin{DataStructure}{Structure \dstr{PSP:}}
+\dusa{PSGEO} \moc{:=} \moc{PSP:} \dusa{PSGEO} $\{$ \dusa{GEONAM} $|$ \dusa{TRKNAM} $\}$ $[$ \dusa{FLUNAM} $]$ \moc{::} \dstr{descpsp}
+\end{DataStructure}
+
+\noindent  where
+\begin{ListeDeDescription}{mmmmmmm}
+
+\item[\dusa{PSGEO}] {\tt character*12} name of the file that will contain the graphical description in a POSTSCRIPT 
+format. This file must have a sequential ASCII format. 
+
+\item[\dusa{GEONAM}] {\tt character*12} name of a read-only {\sc geometry} (see Section \Sect{GEOData}). 
+
+\item[\dusa{TRKNAM}] {\tt character*12} name of an NXT or EXCELL type read-only {\sc tracking} (see Sections.~\ref{sect:EXCELLData}
+and~\ref{sect:NXTData}).
+
+\item[\dusa{FLUNAM}] {\tt character*12} name of an optional read-only {\sc fluxunk} (see \Sect{FLUData}). It is required only 
+if a flux mapping plot is requested. 
+
+\item[\dstr{descpsp}] structure containing the input data to this module (see \Sect{PSPdesc}).
+
+\end{ListeDeDescription}
+
+\subsubsection{Data input for module {\tt PSP:}}\label{sect:PSPdesc}
+
+\begin{DataStructure}{Structure \dstr{descpsp}}
+$[$ \moc{EDIT} \dusa{iprint} $]$ \\
+$[$ \moc{FILL} $\{$ \moc{NONE} $|$ \moc{GRAY} $|$ \moc{RGB} $|$ \moc{CMYK} $|$ \moc{HSB} $\}~[$ \moc{NOCONTOUR} $]~]$ \\
+$[$ \moc{TYPE} $\{$ \moc{REGION} $|$ \moc{MIXTURE} $|$ \moc{FLUX} $|$ \moc{MGFLUX} $\}~]$
+\end{DataStructure}
+
+\noindent where
+
+\begin{ListeDeDescription}{mmmmmmmm}
+
+\item[\moc{EDIT}] keyword used to modify the print level \dusa{iprint}. 
+
+\item[\dusa{iprint}] index used to control the printing in this module. It must be set to 0 if no printing on the output 
+file is required. 
+
+\item[\moc{FILL}] keyword to specify the drawing options. 
+
+\item[\moc{NONE}] keyword to specify that only region contour are to be drawn. 
+
+\item[\moc{GRAY}] keyword to specify that the regions will be filled with various levels of gray. 
+
+\item[\moc{RGB}] keyword to specify that the regions will be filled with various colors taken using the RGB color 
+scheme. 
+
+\item[\moc{CMYK}] keyword to specify that the regions will be filled with various colors taken using the CMYK 
+color scheme. 
+
+\item[\moc{HSB}] keyword to specify that the regions will be filled with various colors taken using the HSB color 
+scheme. This is the default option. 
+
+\item[\moc{NOCONTOUR}] keyword to specify that the contour lines delimiting each region will not be drawn. 
+
+\item[\moc{TYPE}] keyword to specify the type of graphics generated. 
+
+\item[\moc{REGION}] keyword to specify that different colors or gray levels will be associated with each region. This 
+is the default option. 
+
+\item[\moc{MIXTURE}] keyword to specify that different colors or gray levels will be associated with each mixture. 
+
+\item[\moc{FLUX}] keyword to specify that the group integrated flux is to be drawn. 
+
+\item[\moc{MGFLUX}] keyword to specify that the group flux is to be drawn.
+
+\end{ListeDeDescription}
+
+\eject
-- 
cgit v1.2.3

