From 7dfcc480ba1e19bd3232349fc733caef94034292 Mon Sep 17 00:00:00 2001
From: stainer_t <thomas.stainer@oecd-nea.org>
Date: Mon, 8 Sep 2025 13:48:49 +0200
Subject: Initial commit from Polytechnique Montreal

---
 doc/IGE351/SectDdepos.tex | 64 +++++++++++++++++++++++++++++++++++++++++++++++
 1 file changed, 64 insertions(+)
 create mode 100644 doc/IGE351/SectDdepos.tex

(limited to 'doc/IGE351/SectDdepos.tex')

diff --git a/doc/IGE351/SectDdepos.tex b/doc/IGE351/SectDdepos.tex
new file mode 100644
index 0000000..09f2cf4
--- /dev/null
+++ b/doc/IGE351/SectDdepos.tex
@@ -0,0 +1,64 @@
+\section{Contents of a \dir{deposition} directory}\label{sect:depositiondir}
+
+This directory accumulates energy and charge deposition information gathered from coupled solutions of the Boltzmann and/or Boltzmann
+Fokker-Planck transport equations.
+
+\subsection{State vector content for the \dir{deposition} data structure}\label{sect:depositionstate}
+
+The dimensioning parameters for this data structure, stored in the state vector
+$\mathcal{S}^{dep}_{i}$, represent:
+
+\begin{itemize}
+
+\item The number of material mixtures $N_{\rm mix}=\mathcal{S}^{dep}_{1}$
+
+\item The number of particules contributing to deposition $N_{\rm part}=\mathcal{S}^{dep}_{2}$
+
+\item Charge deposition index $I_{\rm c}=\mathcal{S}^{dep}_{3}$:
+\begin{displaymath}
+I_{\rm c} = \left\{
+\begin{array}{ll}
+0 & \textrm{no charge deposition information}\\
+1 & \textrm{charge deposition information is present.}
+\end{array} \right.
+\end{displaymath}
+
+\item The number of Boltzmann transport equation iterations $N_{\rm iter}=\mathcal{S}^{dep}_{4}$
+\end{itemize}
+
+\subsection{The main \dir{deposition} directory}\label{sect:depositiondirmain}
+
+On its first level, the following records and sub-directories will be found in the \dir{deposition} directory:
+
+\begin{DescriptionEnregistrement}{Main records and sub-directories in \dir{deposition}}{6.0cm}
+\CharEnr
+  {SIGNATURE\blank{3}}{$*12$}
+  {Signature of the data structure ($\mathsf{SIGNA}=${\tt L\_DEPOSITION})}
+\IntEnr
+  {STATE-VECTOR}{$40$}
+  {Vector describing the various parameters associated with this data structure $\mathcal{S}^{dep}_{i}$,
+  as defined in \Sect{depositionstate}.}
+\CharEnr
+  {PARTICLE-NAM}{($N_{\rm part}$)$*1$}
+  {Character name associated to each particle.}
+\RealEnr
+  {VOLUME\blank{6}}{$N_{\rm mix}$}{cm$^{3}$}
+  {Volumes.}
+\DbleEnr
+  {FLUX-NORM\blank{3}}{$1$}{$1$}
+  {Flux normalization factor.}
+\DbleEnr
+  {EDEPOS\blank{6}}{$N_{\rm mix},N_{\rm part}$}{MeV$\cdot$cm$^{-3}\cdot$s$^{-1}$}
+  {Energy deposition.}
+\OptDbleEnr
+  {CDEPOS\blank{6}}{$N_{\rm mix},N_{\rm part}$}{$I_{\rm c} = 1$}{electron$\cdot$cm$^{-3}\cdot$s$^{-1}$}
+  {Charge deposition.}
+\DbleEnr
+  {EDEPOS\_TOT\blank{2}}{$N_{\rm mix}$}{MeV$\cdot$cm$^{-3}\cdot$s$^{-1}$}
+  {Volume integrated energy deposition.}
+\OptDbleEnr
+  {CDEPOS\_TOT\blank{2}}{$N_{\rm mix}$}{$I_{\rm c} = 1$}{electron$\cdot$cm$^{-3}\cdot$s$^{-1}$}
+  {Volume integrated charge deposition.}
+\end{DescriptionEnregistrement}
+
+\eject
-- 
cgit v1.2.3

